For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.

#### Preliminary Procedures

Remove the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement.

1 | Steering Wheel Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 30 N·m(22 lb ft)
2 | Steering Wheel

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Loosen the steering wheel bolt until 2 to 3 threads are left engaged.
3. Wiggle the steering wheel until it disengages completely.
4. Remove the steering wheel bolt and steering wheel.