For 1990-2009 cars

#### Special Tools

EN 6009 Remover and Installer Ignition coil

For equivalent regional tools, refer to Special Tools

Note: Note the arrow on the cover.

1. Remove the cover of the ignition coil in the direction of the arrow.
2. Remove the 2 ignition coil bolts
3. Install the EN 6009 remover and installer ignition coil (1)
4. Remove the ignition coil (2).
5. Remove the 11 bolts (2, 3).
6. Remove the camshaft cover (1).