For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the starter motor. Refer to Starter Motor Replacement.

1 | Engine Oil Pressure Switch

#### Procedure

Disconnect the electrial connector.

2 | Engine Oil Pressure Switch Fastener Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a new gasket.