For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove rear seat. Refer to Rear Seat Replacement.
2. Remove the rear seat back. Refer to LINK.
3. Remove the rear compartment access door. Refer to LINK.

1 | Rear Seat Back Cushion Carpet

#### Procedure

1. Loosen out the rear seat back cushion.
2. Clip out the frame door cover.
3. Remove rear seat back cushion carpet.