For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Using a suitable jack stand, support the transmission
2. Remove the battery tray, refer to Battery Tray Replacement.

1 | Transmission Mount Fasteners (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m (16 lb ft)
2 | Transmission Mount Fasteners (Qty: 3)

#### Procedure

Install NEW Bolts.

Tighten
50 N·m (37 lb ft) + 60 degrees + 15 degrees

3 | Transmission Mount - Left Side