For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle

1 | Protective Cover

#### Procedure

1. Remove the protective cover from the hydraulic pump.
2. Disconnect the cable clips.
3. Remove the electrical connection.

2 | Differential Clutch Pump Bolts (Qty: 2) Warning: The hydraulic pressure in the differential clutch is very high. To prevent personal injury, wait for at least 10 minutes before removing any parts from the differential clutch. Caution: Refer to Fastener Caution in the Preface section.

Tighten
6 N·m(53 lb in)

3 | Differential Clutch Pump O-ring (Qty: 2)

#### Procedure

Use new O-rings.

4 | Differential Clutch Pump

#### Procedure

Fill new fluid in the differential clutch. Refer to Adhesives, Fluids, Lubricants, and Sealers