For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the liftgate latch cover. Refer to Liftgate Latch Cover Replacement.
2. Remove the liftgate window side garnish molding. Refer to Liftgate Window Side Garnish Molding Replacement.

1 | Liftgate Trim Finish Panel Fastener
2 | Liftgate Trim Finish Panel Retainer (Qty: 8)
3 | Liftgate Trim Finish Panel Tip Use a BO-569-A plug lifter to aid in the removal of the liftgate trim finish panel.

#### Special Tools

BO-569-A Plug Lifter

For equivalent regional tools, refer to Special Tools