For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front bumper. Refer to Front Bumper Fascia Replacement.
2. Release the air conditioning condenser core and secure it with straps to the vehicle front.

1 | Charge Cooler Pipes

#### Procedure

Detach the charge cooler pipes on both sides.

2 | Power Steering Fluid Cooler

#### Procedure

Release the power steering fluid cooler from the charge cooler and radiator.

3 | Charge Air Cooler