For 1990-2009 cars

1. Install the intake manifold (2).
2. Install the throttle body (1).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 3 throttle body bolts (9) and tighten to XX N·m (XX lb ft).
4. Install the actuating drive-change over bracket (6).
5. Install the 2 actuating drive-change over bracket bolts (7) and tighten to XX N·m (XX lb ft).
6. Install the actuating drive-change over (8).
7. Install the 2 actuating drive-change over bolt (5) and tighten to XX N·m (XX lb ft).
8. Install the manifold absolute pressure sensor (3).
9. Install the manifold absolute pressure sensor bolt (4) and tighten to XX N·m (XX lb ft).