For 1990-2009 cars

Condition | Action
--- | ---
Warning: While engine is operating, the exhaust system will become extremely hot. To prevent burns avoid contacting a hot exhaust system. DEFINITION: An audible or physical noise due to a faulty component or damaged components causing a loose or misaligned exhaust system resulting in a rattle or vibration noise, i.e. buzz, groan, hum.

Refer to Symptoms - Engine Exhaust.

Popping or hissing noise | Exhaust leak--Refer to Exhaust Leakage
Loud exhaust |

1. 1. Compare to a known good vehicle.
2. Inspect for a damaged or failed muffle
3. Replace the faulty muffler. Refer to Exhaust Muffler Replacement

External rattle or vibration noise |

1. Inspect for a bent or loose hanger, loose heat shield, or loose clamp.
2. Inspect for a exhaust pipe causing interference.
3. Repair or replace the affected component. Refer to the affected component's service procedure.

Internal rattle |

1. Test the components by tapping with a rubber mallet to confirm a rattle.
2. Replace the faulty catalytic converter, or muffler. Refer to one of the following procedures:

• | Refer to Exhaust Manifold Replacement or Exhaust Manifold Replacement - Left Side or Exhaust Manifold Replacement - Right Side.

• | Refer to Catalytic Converter Replacement.

• | Refer to Exhaust System Replacement.