For 1990-2009 cars

Callout | Component Name
--- | ---
Note: Ensure that the rear window wiper arm remains at rest position and Does Not spring back onto the rear window.

#### Preliminary Procedure

Raise the rear window wiper arm to the full up position (service up).

1 | Rear Window Wiper Arm
2 | Rear Window Wiper Blade Retainer (Qty: 2)

#### Procedure

Squeeze both retainers and rotate the rear window wiper blade away from the rear window wiper arm to remove.

3 | Rear Window Wiper Blade Tip Discard and replace if rubber appears worn or does not wipe the rear window clean.