For 1990-2009 cars

## Turbocharger Coolant Feed Pipe Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Draining the engine cooling fluid. Refer to LINK.
2. Remove engine appearance cover replacement. Refer to LINK.

1 | Turbocharger Coolant Feed Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use new gasket

Tighten
X N·m (X lb in)

2 | Release the Turbocharger Coolant Feed Pipe. Retainer (Qty: 2)
3 | Turbocharger Coolant Feed Pipe Fastener Tighten X N·m (X lb in)
4 | Turbocharger Coolant Feed Pipe