For 1990-2009 cars

1. Ensure that the crankshaft is in the stage 2 timing drive assembly position (1).
2. Install the secondary timing chain (1).
3. Place the secondary timing chain bank 1 around the timing chain idler sprocket bank 1, aligning the secondary timing chain link (1) with the alignment access hole (2) made in the timing chain idler sprocket bank 1.
4. Wrap the secondary timing chain bank 1 around both camshaft position actuator bank 1.
5. Ensure there are 10 links (1) between the secondary timing chain links for the camshaft position actuator bank 1.
6. Align the exhaust camshaft position actuator bank 1 alignment triangle mark (1) with the secondary timing chain bank 1 link (2).
7. Align the intake camshaft position actuator bank 1 alignment triangle mark (2) with the secondary timing chain bank 1 link (1).
8. There will be 22 links (1) between the timing chain idler sprocket bank 1 and each camshaft position actuators bank 1.