For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the transmission control lever boot. Refer to Transmission Control Lever Boot Replacement.
2. Remove the battery tray. Refer to Battery Tray Replacement.

1 | Inner Shift Cable Clamping Assembly (Qty: 2)

#### Procedure

1. Release selector cable from clamping piece.
2. Remove the 2 shift cables from the counterhold.

#### Procedure

Open clamping piece using a small screwdriver. Open only as far as the notch, opening any further (overstretching) may destroy clamping piece.

2 | Adjustment Position

#### Procedure

1. Pull reverse gear pawl upwards.
2. Compress lugs using pliers until locking block jumps downwards.
3. Secure shift lever in neutral position 1st/2nd gear level with locking block at bracket.

3 | Shift Actuation

#### Procedure

1. Place Transmission in Neutral.
2. Pull Shift Actuation Upwards (Arrow).
3. Secure shift actuation with DT-49544 adjuster , must engage noticeably.
4. To remove DT-49544 adjusting tool , pull shift actuation slightly upwards (arrow).

#### Special Tool

DT-49544 Adjusting Tool

For equivalent regional tools, refer to Special Tools.

4 | Inner Shift Cable Clamping Assembly (Qty: 2)

#### Procedure

1. Lock selector connection clamping piece by compressing. DO NOT move shift lever.
2. Check for easy shifting of gears.

5 | Manual Transmission Shift Lever Cable