For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to Battery Disconnect Warning in the Preface section.

#### Preliminary Procedure

Remove the battery negative terminal. Refer to Battery Negative Cable Disconnection and Connection.

1 | Battery Fuse Cover Plate
2 | Battery Positive Cable Caution: Refer to Fastener Caution in the Preface section. Tighten 8 N·m (70.8 lb in)
3 | Battery Fuse Assembly
4 | Engine Diagnosis Module Retainer Plate

#### Procedure

Release the engine diagnosis module retainer plate and lift upwards.

5 | Battery Retainer Fastener Tighten 10 N·m (89 lb in)
6 | Battery Retainer Bracket Caution: Whenever the brake rotor has been separated from the wheel bearing flange, clean any rust or foreign material from the mating surface of the rotor and flange with the J 42450 hub cleaning kit. Failure to do this may result in increased lateral runout of the rotor and brake pulsation.

#### Procedure

Release the battery retainer plate and lift upwards.

7 | Battery