For 1990-2009 cars

The torque converter stator roller clutch can have two different malfunctions.

1. Inspect the control solenoid (w/body and TCM) valve assembly connectors and pins (A, B, C) for the following conditions:

• | Damage

• | Bent pins

• | Debris

• | Broken retaining tab

• | Contamination

2. Ensure no metallic debris is inside the connectors near the terminal pins.
3. Inspect the control solenoid (w/body and TCM) valve assembly solenoid leads for contamination or metallic debris.
4. Inspect for oil leakage from any of the gaskets.