For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Turn the ignition OFF.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
3. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
4. Remove the air cleaner outlet duct. Refer to Air Cleaner Outlet Duct Replacement.

1 | Secondary Injection Shutoff Valve Pressure Sensor

#### Procedure

1. Remove both fasteners.
2. Disconnect the electrical connector.

2 | Secondary Air Injection Outlet Pipe

#### Procedure

Disconnect both quick connectors.