For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the left side instrument panel lower trim panel. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side.
2. Remove the steering column upper trim cover from the instrument panel. Refer to Steering Column Trim Cover Replacement.

1 | Instrument Cluster Assembly Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Instrument Cluster Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Remove the instrument cluster.
3. For programming and set up information refer to Control Module References.