For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Remove the trailing arm. Refer to Trailing Arm Replacement.

1 | Trailing Arm Bushing

#### Procedure

Adjust bushing 18.7 mm from center of hole, when parralell to bushing console with the CH-49381 kit .

#### Special Tools

CH-49381 Remover Installer Kit