For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement.

1 | Outside Rearview Mirror Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Disconnect the mirror electrical connector.

Tighten
9 N·m (80 lb in)

2 | Outside Rearview Mirror Assembly Tip The mirror assembly must be ordered and assembled prior to being installed to the vehicle.