For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: The steering column must be in the LOCK position before disconnecting the following components:

• | The steering column

• | The steering shaft coupling

• | The intermediate shaft

• | The lower steering shaft

After disconnecting these components, do not move the front tires and wheels. Failure to follow these procedures may cause improper alignment of some components during installation and result in possible damage to the SIR coil.

#### Preliminary Procedures

1. Remove the left side instrument panel lower trim panel insulator. Refer to Instrument Panel Lower Trim Panel Insulator Replacement.
2. Remove the lower steering column trim cover. Refer to Steering Column Trim Cover Replacement.
3. Disconnect the intermediate steering shaft from the steering gear. Refer to Steering Gear Replacement.

1 | Steering Column Nut (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 22 N·m(16 lb ft) + 30 degrees
2 | Steering Column

#### Procedure

1. Disconnect any electrical connectors as needed.
2. Transfer any parts as needed.
3. After installation center the steering angle sensor. Refer to Steering Angle Sensor Centering.