For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Lower the front of the headlining trim panel to access the sunshade electrical connector, if necessary.

1 | Sunshade Support Fastener Cover
2 | Sunshade Fastener (Qty: 3)
3 | Sunshade Assembly

#### Procedure

1. Disconnect the electrical connector.
2. Remove the sunshade anchor from the roof by unsnapping, if needed.