For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove floor air outlet duct. Refer to Floor Air Outlet Duct Replacement - Right Side.
3. Disconnect the heater and blower and air conditioning control module electrical connectors.

1 | Heater and Blower and Air Conditioning Control Module Fastener (Qty: 2)
2 | Heater and Blower and Air Conditioning Control Module