For 1990-2009 cars

1. Install the catalytic converter (4).
2. Install a NEW clamp (2) to connect the catalytic converter (4) and the exhaust pressure sensor pipe (2).
3. Install the 2 catalytic converter brace bracket studs (6).

Caution: Refer to Fastener Caution in the Preface section.

4. Install the 2 catalytic converter brace bracket nuts (5) and tighten to 20 N·m (15 lb ft).
5. Install the clamp assembly catalytic converter (3) and tighten to XX N·m (XX lb in).