For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front tire and wheel assemblies.

1 | Electronic Suspension Front Position Sensor Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 9N·m (80 lb in)
2 | Electronic Suspension Front Position Sensor

#### Procedure

1. Remove the connector from the strut.
2. Disconnect the connector from the sensor, the connector has a secondary locking mechanism that should be released before turning and releasing the connector.