For 1990-2009 cars

## Rear Axle Shaft Seal Replacement - Right Side Right Side

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the right rear wheel drive shaft. Refer to Rear Wheel Drive Shaft Replacement

1 | Rear Axle Shaft Seal

#### Procedure

Check lubricant level. Refer to Rear Axle Lubricant Level Inspection

#### Special Tools

• | DT-49536 Puller, drive shaft seal

• | DT-49537 Puller

• | DT-49068 Fitting drift

For equivalent regional tools, refer to Special Tools