For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the catalytic converter. Refer to Catalytic Converter Replacement.

1 | Turbocharger Oil Return Pipe Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a new gasket.

Tighten
10 N·m (89 lb in)

2 | Turbocharger Oil Return Pipe

#### Procedure

Pull the turbocharger oil return hose out from the engine block.