For 1990-2009 cars

## Engine Coolant Air Bleed Hose Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---
1 | Engine Coolant Air Bleed Hose
2 | Engine Coolant Air Bleed Hose

## Engine Coolant Air Bleed Hose Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Drain the cooling system. Refer to Cooling System Draining and Filling.

1 | Engine Coolant Air Bleed Hose Retainer (Qty: 2)

## Engine Coolant Air Bleed Hose Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the engine cover. Refer to Engine Cover Replacement.

1 | Engine Coolant Air Bleed Hose.

#### Procedure

1. Release the hose clip from the surge tank and detach the hose.
2. Release the hose clip from the engine and detach the bleed hose.
3. After installation, fill the cooling system. Refer to Cooling System Draining and Filling.
4. After repairs, inspect the cooling system for leaks.