For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Drain the engine oil. Refer to LINK.
2. Remove the oil level indicator. Refer to LINK.
3. Remove the exhaust muffler. Refer to Exhaust Muffler Replacement.

1 | Oil Pan Fastener (Qty: 15) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)
2 | Oil Pan
3 | Oil Pan Baffle Fastener Tighten X N·m (X lb in)
4 | Oil Pan Baffle
5 | Oil Level Sensor Fastener (Qty: 2) Tighten X N·m (X lb in)
6 | Oil Level Sensor