For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.

1 | Stabilizer Shaft Link Fastener (Qty: 2) Caution: Refer to Fastener Caution in the Preface section. Tighten 50 N·m(37 lb ft)
2 | Stabilizer Shaft Link