For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the driver knee bolster. Refer to Link.
2. Release the electrical connector.

1 | Ac celerator Pedal Fastener Caution: Refer to Fastener Caution in the Preface section. Tighten 3.5 N·m 36 lb in
2 | Accelerator Pedal Assembly

#### Procedure

1. Twist the accelerator pedal upwards.
2. Move the accelerator pedal downwards.
3. Remove the Accelerator pedal.

3 | Accelerator Pedal Position Sensor

#### Procedure

Release the retainers to remove the accelerator pedal position sensor.