For 1990-2009 cars

## Air Inlet Valve Actuator Replacement Left Hand Drive and CJ2

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel (I/P) lower extension side trim panel. Refer to Instrument Panel Lower Extension Side Trim Panel Replacement.
3. Remove temperature valve actuator - right side. Refer to Temperature Valve Actuator Replacement - Right Side.
4. Remove the heater and blower and air conditioning control module. Refer to Heater and Blower and Air Conditioning Control Module Replacement.

1 | Recirculation Actuator Fastener (Qty: 3)

#### Procedure

Disconnect the recirculation actuator electrical connector.

2 | Recirculation Actuator Tip Actuator is self-calibrating when connecting the battery.