For 1990-2009 cars

## Outside Mirror Description and Operation w/A45

### Power Mirror System Components

The power mirror system consists of the following components:

• | Memory Seat Module

• | Outside Mirror Switch

• | Passenger Window Switch

• | Left Outside Rearview Mirror

• | Right Outside Rearview Mirror

### Power Mirror System Controls

The outside mirror switch and passenger window switch are on a serial data circuit with the memory seat module as the master. The mirror select and directional control switches are inputs to the memory seat module through the serial data circuit. When the memory seat module receives switch inputs from the outside mirror switch, mirror output commands are sent to the appropriate switch through the serial data circuit. The outside mirror switch and passenger window switch control the left and right outside rear view mirrors through bi-directional motor control circuits. The motor control circuits are floating while in an inactive state and the switches will apply power and ground to the control circuits as necessary to move the mirror in the commanded direction.

Mirror position is determined by both horizontal and vertical position sensors in each of the power mirrors. The outside mirror switch and passenger window switch supply a 5 V reference, low reference, and horizontal and vertical position signal circuits to these sensors. The signal circuits are referenced from 5 V by the switches and the signal circuit voltage levels represent the mirror positions. The mirror positions are sent to the memory seat module through the serial data circuit where they are stored for memory mirror operation. When the memory seat module receives a memory recall command, the memory seat module will send the go to position commands to the outside mirror switch and passenger window switch. The switches will then drive the appropriate mirror motors to the commanded position sensor settings.

### Folding Mirrors

The mirror select and fold/retract switches are inputs to the memory seat module through a serial data circuit. When the memory seat module receives a fold or retract signal from the outside mirror switch the memory seat module will send a fold or retract command to the outside mirror switch and passenger window switch. The outside mirror switch and passenger window switch control the fold/retract motors through bi-directional control circuits.

This function can also be achieved through the Comfort Open/Close function. If enabled through personalization, the Comfort Open will retract the mirrors and Comfort Close will fold the mirrors.

### Heated Mirrors

The heated mirrors are controlled through the rear defog relay. Whenever the rear window defogger is turned on battery voltage is supplied to the mirror heater elements through the left and right mirror heater element control circuits.

## Outside Mirror Description and Operation w/o A45

### Power Mirror System Components

The power mirror system consists of the following components:

• | Mirror direction switch -- Controls the left, right, up and down movements of the mirrors

• | Mirror select switch -- Allows the operator to select the mirror to be moved

• | Left outside mirror -- Contains both the horizontal and vertical mirror motors

• | Right outside mirror -- Contains both the horizontal and vertical mirror motors

Each of the outside power mirrors contains 2 motors. The up-down motor operates the vertical directions and the left-right motor operates the horizontal directions. Each of the power mirror motors are internally circuit breaker protected.

### Power Mirror System Controls

The outside mirror switch incorporates a mirror select switch and a 4 position mirror direction switch.

The mirror select switch allows the driver to select the mirror to be moved by pressing the switch to L position enabling the left outside mirror or pressing the switch to R position enabling the right outside mirror.

The mirror direction switch is a 4 position switch that allows the operator to move the selected mirror up, down, left or right.

### Power Mirror System Operation

The outside mirror switch receives power through the battery positive voltage circuit from the underhood fuse block. The outside mirror switch also receives a constant ground.

The 4 positions of the direction switch have multiple switch contacts. When not in use, the directional contacts are isolated from any circuit. Each of the contacts are connected to opposing sides of the appropriate mirror motors through the selector switch. The selector switch interrupts or completes these circuits depending on the position of the selector switch, L or R.

If the mirror select switch is placed in the L position and the up switch is pressed, battery voltage will be supplied to the driver outside mirror vertical motor through the driver mirror motor up control circuit and return to the mirror switch through the driver mirror motor left/down control circuit, then to ground and the mirror will move up. If the down switch is pressed, the driver mirror motor left/down control circuit supplies battery voltage and the driver mirror motor up control circuit completes the path to the mirror switch, then to ground and the mirror will move down.

The remainder of the mirror functions operate in the same manner as described above. Placing the mirror control switch in opposing positions, left/right or up/down, will reverse the voltage polarity to the mirror motor, utilizing the same circuits and the mirror will move accordingly.