For 1990-2009 cars

## Water Pump Removal LDK

1. Remove the engine coolant temperature sensor (1).
2. Remove the thermostat and water feed pipe retaining bolts.

Note: Twist the water feed pipe while pulling to remove it from the water pump cover.

3. Remove the thermostat housing (1) and water feed pipe (2) from the water pump cover.
4. Remove the water pump retaining bolts. Be sure to remove the bolt that goes through the front of the engine block.
5. Remove the water pump assembly (1).
6. Remove and discard the gasket (2).