For 1990-2009 cars

## Duct Air Temperature Sensor Replacement - Upper Right Side Left Hand Drive and CJ2

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument panel (I/P) lower extension side trim panel. Refer to Instrument Panel Lower Extension Side Trim Panel Replacement.
3. Remove the temperature valve actuator - right side. Refer to Temperature Valve Actuator Replacement - Right Side.
4. Remove the heater and blower and air conditioning control module. Refer to Heater and Blower and Air Conditioning Control Module Replacement.
5. Remove the recirculation actuator. Refer to Recirculation Actuator Replacement.

1 | Air Temperature Sensor - Upper Right Side

#### Procedure

1. Disconnect the air temperature sensor electrical connector.
2. Twist and pull the upper air temperature sensor from the HVAC module assembly.