For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Engine Control Module Retainer (Qty: 3)

#### Procedures

1. Disconnect the electrical connector.
2. Pull up the engine control module from the battery box.
3. Open with caution both retainers at the sides and pull the engine control module outside the bracket.

2 | Engine Control Module

#### Procedure

Refer to Control Module References for programming and set up of the engine control module.