For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the rear side door water deflector. Refer to Rear Side Door Water Deflector Replacement.
2. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

1 | Rear Side Door Wiring Harness Retainer (Qty: 12)
2 | Rear Side Door Wiring Harness

#### Procedure

Disconnect the electrical connector.