For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle

• | Review Strategy Based Diagnosis

• | Diagnostic Procedure Instructions

### Circuit/System Description

The engine control module (ECM) enables the fuel pump relay when the ignition switch is turned ON. The ECM will disable the fuel pump relay within 2 s unless the ECM detects crankshaft reference pulses. The ECM continues to enable the fuel pump relay as long as crankshaft reference pulses are detected. The ECM disables the fuel pump relay within 2 s if crankshaft reference pulses cease to be detected and the ignition remains ON.

The fuel tank stores the fuel supply. An electric fuel pump attaches to the fuel pump module inside the fuel tank. Fuel flows to the fuel filter/heater element housing , which combines a water separator, fuel heater element, and a filter element. The fuel is then delivered to the high-pressure pump. The mechanical fuel injection pump is located at the front of the engine. The mechanical fuel injection pump is engine-driven by the timing belt. From the high-pressure pump, the pressurized fuel flows to the fuel rail. The fuel rail is equipped with a fuel rail pressure sensor and a fuel pressure regulator.

The fuel return system returns not used fuel to the fuel tank. Fuel is used to cool and lubricate the fuel injectors and fuel injection pump. If the high side fuel pressure becomes excessive, the fuel pressure regulator releases the fuel into the fuel return system. The return fuel travels through the fuel lines and then to the fuel tank.

### Diagnostic Aids

A Cranks But Will Not Run or Hard Start symptom may exist if air is being drawn into the fuel injection system due to the following conditions:

• | Deformed or cut O-rings at the fuel supply line connections

• | Improperly seated fuel supply line fittings

• | Porous or weathered rubber fuel supply lines

• | Fuel filter vent screw not tighten or cross threaded

• | Fuel filter not tighten properly

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Description and Operation

Fuel System Description

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### Scan Tool Reference

Control Module References

### Circuit/System Verification

Note:

• | Inspect the fuel system for damage or external leaks before proceeding.

• | Verify that adequate fuel is in the fuel tank before proceeding.

1. Ignition ON, command the Fuel Pump Relay ON and OFF with a scan tool. You should hear the fuel pump turn ON and OFF.

⇒ | If the fuel pump does not turn ON, refer to Fuel Pressure Gage Installation and Removal

2. Observe the scan tool Fuel Rail Pressure Sensor parameter. During engine cranking, the pressure should be at least 415 kPa (60 PSI). With the engine running at idle the pressure should be close to the Desired Fuel Rail Pressure parameter. As the engine speed is increased, the Desired Fuel Rail Pressure parameter and the Fuel Rail Pressure Sensor parameter should closely match each other.

### Circuit/System Testing

Note: It may be necessary to remove engine components for the visual inspections.

1. Verify the following conditions do not exist:

• | Hoses and lines that are flattening when the engine is running, or have kinks that may restrict the flow of fuel

• | Fuel leaks between the fuel tank and the fuel injection pump

| Note: A fuel return line that is leaking , is a good indication there is a restriction in the return system.

• | Fuel leaks in the fuel return lines

⇒ | Repair any leaks, restrictions, or replace any components found to be damaged or leaking.

2. Install the fuel pressure gage. Refer to Fuel Pressure Gage Installation and Removal

Note: The fuel pump relay may need to be commanded ON a few times in order to obtain the highest possible fuel pressure.

3. Ignition ON, command the fuel pump relay ON with a scan tool. Verify the fuel pressure is between 415-535 kPa (60-78 PSI) and remains steady for 5 minutes.

⇒ | If less than the specified range, remove the fuel tank and test, inspect, and repair the items listed below. If all items test normal, replace the fuel pump.

• | Leaking fuel lines

• | Restricted fuel feed pipe

• | Restricted or plugged strainer

• | Stuck or binding fuel level float

• | Inspect the harness connectors and the ground circuits of the fuel pump for poor connections.

4. If the fuel system components test normal, test or replace the fuel filter.

### Repair Instructions

Perform the Diagnostic Repair Verification

• | Fuel Filter Replacement

• | Fuel Tank Replacement