For 1990-2009 cars

#### Special Tools

• | EN-6347 Holder

• | EN-956-1 Extension

• | EN-46790 Fuel Injection Pump Sprocket Remover

For equivalent regional tools, refer to Special Tools.

1. Install the EN-6347 fuel injection pump sprocket holder (1) with EN-956-1 tool extension (2) to the fuel injection pump driven sprocket.
2. Remove the fuel injection pump driven sprocket nut.
3. Remove the EN-6347 holder with EN-956-1 extension to the fuel injection pump driven sprocket.
4. Install the EN-46790 fuel injection pump sprocket remover (1).
5. Remove the fuel injection pump driven sprocket with EN-46790 fuel injection pump sprocket remover .