For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Front Seat Head Restraint Guide Bezel
2 | Securing’s Front Seat Head Restraint Adjust Rod Guide
3 | Front Seat Head Restraint

#### Procedures

1. Open cushion cover at front seat - rear side.
2. Cut cable strap from the bowden cable head restraint.
3. Clip out bowden wire of head restraint - right side.
4. Clip out bowden wire of head restraint - left side.
5. Release both head restraint guide bezel.
6. Remove both securing’s of head restraint adjust rod guide.
7. Remove front seat head restraint.
8. Install new front seat head restraint adjust rod guide.

Tip
Use commercial screwdriver to remove both of the securing head restraint adjust rod guide.