For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Raise the vehicle by its full height. Refer to Lifting and Jacking the Vehicle.

1 | Exhaust Front Pipe Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb ft)
2 | Exhaust Front Pipe Fastener (Qty: 2) Tighten X N·m (X lb ft)
3 | Exhaust Front Pipe Fastener (Qty: 2) Tighten X N·m (X lb ft)
4 | Exhaust Front Pipe