For 1990-2009 cars

## Air Conditioning Refrigerant Temperature Sensor Replacement Left Hand Drive

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove instrument panel (I/P) compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the floor air outlet duct - right side. Refer to Floor Air Outlet Duct Replacement - Right Side.

1 | Air Conditioning Refrigerant Temperature Sensor

#### Procedure

1. Disconnect the refrigerant temperature sensor electrical connector.
2. Twist and pull the refrigerant temperature sensor from the HVAC module assembly.

## Air Conditioning Refrigerant Temperature Sensor Replacement Left Hand Drive and CJ2

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove instrument panel compartment. Refer to Instrument Panel Compartment Replacement.
2. Remove the floor air outlet duct - right side. Refer to Floor Air Outlet Duct Replacement - Right Side.

1 | Air Conditioning Refrigerant Temperature Sensor

#### Procedure

1. Disconnect the refrigerant temperature sensor electrical connector.
2. Twist and pull the refrigerant temperature sensor from the HVAC module assembly.