For 1990-2009 cars

## Compressor Pressure Relief Valve Replacement LBW/A28NET

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
2. Remove Charge Air Cooler Outlet Hose assembly. Refer to Charge Air Cooler Outlet Hose Replacement.

1 | Compressor Pressure Relief Valve Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)

## Compressor Pressure Relief Valve Replacement LDE/A16XER, 2H0/A18XER

Callout | Component Name
--- | ---

#### Preliminary Procedure

Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.

1 | Compressor Pressure Relief Valve Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)

## Compressor Pressure Relief Valve Replacement LDK/A20NHT

Callout | Component Name
--- | ---

#### Preliminary Procedure

Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.

1 | Compressor Pressure Relief Valve Caution: Refer to Fastener Caution in the Preface section. Tighten X N·m (X lb in)

## Compressor Pressure Relief Valve Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.

1 | Compressor Pressure Relief Valve Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Use a new O-ring.

Tighten
10 N·m(89 lb in)