For 1990-2009 cars

#### Special Tools

EN 46789 Camshaft Fixing Tool

For equivalent regional tools, refer to Special Tools.

1. Install the exhaust camshaft (2).
2. Install the exhaust camshaft sealing ring (1).
3. Install the EN 46789 fixing tool .
4. Install the exhaust camshaft sprocket (1).

Caution: Refer to Fastener Caution in the Preface section.

5. Install the exhaust camshaft sprocket bolt (2) and tighten to XX N·m (XX lb ft).