For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the catalytic converter. Refer to Catalytic Converter Replacement.

1 | Exhaust Manifold Heat Shield Rear Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Heater Outlet Pipe Fastener Tighten 62 N·m (46 lb ft)
3 | Heater Outlet Pipe Tip Do NOT remove the heater outlet pipe from the vehicle. Install a NEW O-ring.
4 | Exhaust Manifold Brace Fastener (Qty: 3) Tighten 30 N·m (22 lb ft)
5 | Exhaust Manifold Brace
6 | Exhaust Turbocharger Inlet Pipe Fastener (Qty: 2) Tighten 30 N·m (22 lb ft)
7 | Exhaust Turbocharger Inlet Pipe Tip Use NEW gaskets.
8 | Bank 1 Exhaust Manifold

#### Procedure

1. Remove the bank 1 exhaust manifold. Refer to Exhaust Manifold Removal - Bank 1.
2. Install the bank 1 exhaust manifold. Refer to Exhaust Manifold Installation - Bank 1.