For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation.
2. Remove the steering gear boot. Refer to Steering Gear Boot Replacement - On Vehicle.

1 | Steering Linkage Inner Tie Rod Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Place a wrench on the flats of the steering linkage inner tie rod housing.
2. Rotate the steering linkage inner tie rod housing counterclockwise until the steering linkage inner tie rod separates from the rack.
3. Remove the old locking agent from the threads of the rack and the steering linkage inner tie rod.
4. Apply locking agent to the steering linkage inner tie rod threads. Refer to Adhesives, Fluids, Lubricants, and Sealers for the recommended threadlock material.
5. Adjust the front toe. Refer to Wheel Alignment - Steering Wheel Angle and/or Front Toe Adjustment.

Tip
A 2.5 mm shim is used for vehicles with wheels up to 18 inches and a 5.6 mm shim is used for vehicles with 19 inch and 20 inch wheels.

Tighten
35 N·m (26 lb ft)