For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Position the window approximately half-way down in the door.
2. Remove the front side door water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Remove the front side door window outer sealing strip. Refer to Front Side Door Window Outer Sealing Strip Replacement.
4. Release the left and right front side door window weatherstrip, if necessary. Refer to Front Side Door Window Weatherstrip Replacement.

1 | Front Side Door Window Retainer (Qty: 2)
2 | Front Side Door Window

#### Procedure

1. Using mask tape, tape off the outer door frame to prevent scratches.
2. Loosen the window regulator sash tabs, pull upward to release the front side door window from the sash.
3. Rotate the front side door window as necessary to remove it from the door.