For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

Remove the water deflector. Refer to Front Side Door Water Deflector Replacement

1 | Front Side Door Outside Handle Rod Retainer Tip Use a flat-head tool to open the retainer from the threaded rod connecting the lock to the outside handle.
2 | Front Side Door Outside Handle Rod

#### Procedure

1. Position the front side door outside handle rod in the retainer in order to eliminate any free play in the outside door handle.
2. Adjust the travel of the handle by removing the threaded rod from the retainer.
3. Install the retainer cover closed over the threaded front side door outside handle rod.
4. Inspect the door lock system for proper operation.