For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.

1 | Rear Side Door Lock Fastener (Qty: 3) Tighten 9 N·m (80 lb in)
2 | Rear Side Door Lock Assembly

#### Procedure

1. Release the shift linkage lever clip.
2. Disconnect the door lock electrical connector.