For 1990-2009 cars

## Battery Tray Replacement Diesel

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the battery. Refer to Battery Replacement.
2. Remove the engine control module with bracket from battery tray.

1 | Glow Plug Relay

#### Procedure

Remove the relay with bracket from the battery tray.

2 | Battery Tray Fastener (Qty: 4) Tighten 25 N·m(18 lb ft)
3 | Battery Tray

#### Procedure

Remove servo oil pipe from battery tray clips.

## Battery Tray Replacement LDE / A16XER, 2HO / A18XER, LDK / A20

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the battery. Refer to Battery Replacement.

1 | Battery Tray Fastener (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 20 N·m (15 lb ft)
2 | Battery Tray

#### Procedure

Transfer any parts as needed.